RFAnalyser v4.8.9 New Features

Ships with version 74 of unit firmware

-	Changes in product configuration file default settings have been carried out.
-	Product functionality changes have been carried out where necessary.
-	Product variants for the Netherlands have been revised to support the allowed bands of operation in that market as specified in the regulations for that country.  
-	Product variants for India have been revised to support the allowed bands of operation in that market as specified in the regulations for that country.
- 	Separate binaries for Indian and Netherlands product variants now added in RFAnalyser.

RF Analyser enhancements

-	RFAnalyser updates have been carried out as follows: 
o	Australian product variant WaveSprint (WM271AU) supports only bands “B” and “C”. Product limited to max 14dbm at port.
o	WaveSprint (WM301AU) supports specified wireless modes for that market.
o	UK Standalone variant support either 2.4GHz or 5GHz wireless modes.
o	Netherlands product variants limited to bands “A” & “B” support to conform to regulations for that market..
o	India product variants include band “D” support to conform to regulations for that market.
-	Software now includes an updated naming convention of firmware to match product codes.
Bug Fixes

-	Classless Inter-Domain Routing (CIDR) now supported (Fixed Subnet bug).
-	Super User Key generator bug now fixed.
-   Alternating bands of operation bug now fixed. e.g. Bands A and B can be enabled without enabling band C.
-   Production test window will not open for paired units.

RF Analyser v4.8.8 New Features

Ships with version 74 of unit firmware

New variants of WaveSprint are added in this version.
-	WaveSprint 5GHz (WM301AU & WM271AU).

RF Analyser enhancements

-	RF Anlayser is now compatible with Windows Vista OS.
-	RF Analyser is ready to operate seamlessly with 
o	WaveSprint variants (WM301AU & WM271AU).

RF Analyser v4.8.7 New Features

Ships with version 72 of unit firmware

The firmware now supports WaveSprint 2.4 GHz V2 and WaveSprint 5.8 GHz V2 product in addition to all of the existing product range. 
All three Band (a,b,c) are enabled by default for WaveSprint 58 and WaveSprint 5.8 GHz V2 product .

Rf Analyser v4.8.6 New Features

Ships with version 70 of unit firmware

The firmware now supports the WaveFlow standalone product in addition to all of the existing product range.

The firmware fixes the following bugs:
-    Scan Subnets icon shown inconsistently.

Rf Analyser v4.8.5 New Features

Ships with version 69 of unit firmware

The firmware now supports the WaveSprint standalone product in addition to all of the existing product range.

The firmware fixes the following bugs:
-    Scan Subnets icon shown inconsistently.

Rf Analyser v4.8.4 New Features

Ships with version 68 of unit firmware

This firmware has the following features:

-     Access Point Capability information expanded to allow all third-party clients.
-	Rx Errors no longer include PhyErrors from the Atheros chip. PhyErrors include false locks which distort the error count as this does not indicate a poor link.

The firmware fixes the following bugs:

-     Some system reboot commands operate immediately despite flash writing taking place on the unit for firmware updates.
-	In instances where a logged-in satellite is powered down for a number of minutes, the base can no longer use that login slot for another unit without it being rebooted. In WaveSprint, this means that the satellite cannot log back in after it has been powered down for a number of minutes. 

Rf Analyser Bug Fixes

The following bugs have been fixed in this release:

-	On boards operating in noisier environments, some of the background settings are prone to cause the unit to reboot to move away from the noise. Rf Analyser now sets this setting to increase noise immunity. To “cure” a unit that is suffering from this, simply right click on it, select configure and then save the configuration back to the unit.

Rf Analyser v4.8.3 New Features

Integrated Codec Ready

Rf Analyser is ready to operate seamlessly with the WaveMax Integrated Radio Codec that will ship later in 2007.

Rf Analyser Bug Fixes

The following bugs have been fixed in this release:

-	Some board versions show unstable RSSI due to Antenna mode defaulting to diversity instead of fixed.
-	Unit Passwords were remembered across Rf Analyser sessions by design.

Rf Analyser v4.8.2 New Features

Linux-based WaveMax Ready

Rf Analyser is ready to operate seamlessly with the Linux-based WaveMax products (replacing VxWorks-based ones) that will be shipping later in 2007.

Rf Analyser Bug Fixes

The following bugs have been fixed in this release:

-	On slow connections (such as over a satellite internet connection), configuration write tftp times out and suffers ICMP port unreachable errors.
-	Version 64 of firmware fixed link distance bug, which was limiting achievable link distances to just over 20 km. Rf Analyser now limits the setting according to firmware version.

Rf Analyser v4.8.1 New Features

New Tx Power Maximum for Integrated type units

In response to Ofcom increasing the 5.8GHz maximum power to 4W, the maximum Tx Power for all integrated style units has been increased by 3dB.

WaveMax Single Port Standalone Ready

Rf Analyser is ready to operate seamlessly with the new WaveMax Single Port Standalone product that is shipping later in 2007.

WaveMax Integrated v2.0 Ready

Rf Analyser is ready to operate seamlessly with the new WaveMax Integrated product that is shipping later in 2007.

Bug Fixes

The following bugs have been fixed in this release:

-	Link Diagnostic graph display sometimes halted over long periods of use despite the throughput still being supplied.

Rf Analyser v4.8.0 New Features

New Troubleshooting Guide

Rf Analyser now ships with a troubleshooting guide to help users with installation issues, unit and network settings. It contains a checklist of the most common scenarios that users come across when integrating Wavesight equipment into their networks. The troubleshooting guide can be accessed by clicking on Help->Troubleshooting Guide from the main menu on the Rf Analyser main screen.

Multi Interface Aware

Rf Analyser is now able to operate using any of your PCs network interfaces (provided it is properly assigned an IP Address). It can also cater for multiple IP Addresses on an interface. On start up, Rf Analyser will determine if there are multiple interfaces or IP Addresses and ask the user which they would like to operate from. Provided the equipment is within the same subnet range as the selected IP Address and physically connected to the interface directly or through a network, it will be able to communicate with the device.

WaveFlow v2.0 Ready

Rf Analyser is ready to operate seamlessly with the new WaveFlow product that is shipping later in 2007.

Bug Fixes

The following bugs have been fixed in this release.

-	Configuration files of a size 1 byte over 4kB would be incorrectly interpreted by the unit and could result in incorrect settings being saved.
-	Configuration file uploads whose last packet was incorrectly received by the unit (i.e. lost over the network) would still result in the unit attempting to finalise configuration.
-	Some non-English versions of windows would mangle the contents of Set IP Packets and prevent units from being able to have a new IP Address set.